(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "1_PORT" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 0 7.62 0))
    (property "Value" "1_PORT" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at -1.27 -4.445 0))
    (property "Datasheet" "" (id 3) (at 1.27 5.08 0))
    (property "ki_keywords" "n-ports" (id 4) (at 0 0 0))
    (property "ki_description" "1-port network" (id 5) (at 0 0 0))
    (symbol "1_PORT_0_1")
    (symbol "1_PORT_1_1"
      (pin input line (at -8.89 3.81 0) (length 2.54)
        (name "1+")
        (number "1")
      )
      (pin input line (at -8.89 -3.81 0) (length 2.54)
        (name "1-")
        (number "2")
      )
    )
  )
  (symbol "2_PIN" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 0 4.445 0))
    (property "Value" "2_PIN" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at -1.27 -7.62 0))
    (property "Datasheet" "" (id 3) (at 1.27 1.905 0))
    (property "ki_keywords" "n-pins" (id 4) (at 0 0 0))
    (property "ki_description" "2-pin component" (id 5) (at 0 0 0))
    (symbol "2_PIN_0_1")
    (symbol "2_PIN_1_1"
      (pin input line (at -8.89 0 0) (length 2.54)
        (name "+")
        (number "1")
      )
      (pin input line (at 8.89 0 180) (length 2.54)
        (name "-")
        (number "2")
      )
    )
  )
  (symbol "2_PORT" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 0 7.62 0))
    (property "Value" "2_PORT" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at -1.27 -4.445 0))
    (property "Datasheet" "" (id 3) (at 1.27 5.08 0))
    (property "ki_keywords" "n-ports" (id 4) (at 0 0 0))
    (property "ki_description" "2-port network" (id 5) (at 0 0 0))
    (symbol "2_PORT_0_1")
    (symbol "2_PORT_1_1"
      (pin input line (at -8.89 3.81 0) (length 2.54)
        (name "1+")
        (number "1")
      )
      (pin input line (at -8.89 -3.81 0) (length 2.54)
        (name "1-")
        (number "2")
      )
      (pin input line (at 8.89 3.81 180) (length 2.54)
        (name "2+")
        (number "3")
      )
      (pin input line (at 8.89 -3.81 180) (length 2.54)
        (name "2-")
        (number "4")
      )
    )
  )
  (symbol "3_PIN" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 0 3.81 0))
    (property "Value" "3_PIN" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at -1.27 -7.62 0))
    (property "Datasheet" "" (id 3) (at 1.27 1.905 0))
    (property "ki_keywords" "n-pins" (id 4) (at 0 0 0))
    (property "ki_description" "3-pin component" (id 5) (at 0 0 0))
    (symbol "3_PIN_0_1")
    (symbol "3_PIN_1_1"
      (pin input line (at -8.89 0 0) (length 2.54)
        (name "+")
        (number "1")
      )
      (pin input line (at 8.89 0 180) (length 2.54)
        (name "-")
        (number "2")
      )
      (pin output line (at 0 -5.08 90) (length 2.54)
        (name "out")
        (number "3")
      )
    )
  )
  (symbol "CAP" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (id 0) (at -3.81 0 90))
    (property "Value" "CAP" (id 1) (at -6.35 0 90))
    (property "Footprint" "" (id 2) (at 0.9652 -3.81 90))
    (property "Datasheet" "" (id 3) (at -3.81 0 90))
    (property "c" "<capacitance>" (id 4) (at 3.81 0 90))
    (property "ki_description" "Built-in capacitor" (id 5) (at 0 0 0))
    (symbol "CAP_0_1")
    (symbol "CAP_1_1"
      (pin passive line (at 0 3.81 270) (length 2.794)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -3.81 90) (length 2.794)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "CAP_SEMI" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "C" (id 0) (at -6.35 0 90))
    (property "Value" "CAP_SEMI" (id 1) (at -11.43 0 90))
    (property "Footprint" "" (id 2) (at 0.9652 -3.81 90))
    (property "Datasheet" "" (id 3) (at 0.635 2.54 90))
    (property "Model" "<model name>" (id 4) (at -3.81 0 90))
    (property "w" "<w>" (id 5) (at 3.81 0 90))
    (property "l" "<l>" (id 6) (at 6.35 0 90))
    (property "m" "<m>" (id 7) (at -8.89 0 90))
    (property "ki_description" "Built-in semiconductor capacitor" (id 8) (at 0 0 0))
    (symbol "CAP_SEMI_0_1")
    (symbol "CAP_SEMI_1_1"
      (pin passive line (at 0 3.81 270) (length 2.794)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -3.81 90) (length 2.794)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "CCCS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "F" (id 0) (at 0 5.08 0))
    (property "Value" "CCCS" (id 1) (at 0 7.62 0))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 0))
    (property "gain" "<gain>" (id 4) (at 6.35 0 90))
    (property "Ctlvsrc" "<controlling vsrc>" (id 5) (at -5.08 0 90))
    (property "ki_description" "Built-in current-controlled current source" (id 6) (at 0 0 0))
    (symbol "CCCS_0_0")
    (symbol "CCCS_1_1"
      (pin passive line (at 2.54 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 2.54 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
    )
  )
  (symbol "CCVS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "H" (id 0) (at 0 5.08 0))
    (property "Value" "CCVS" (id 1) (at 0 7.62 0))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 0))
    (property "gain" "<gain>" (id 4) (at 6.35 0 90))
    (property "Ctlvsrc" "<controlling vsrc>" (id 5) (at -5.08 -1.27 90))
    (property "ki_description" "Built-in current-controlled voltage source" (id 6) (at 0 0 0))
    (symbol "CCVS_0_0"
      (text "+" (at 2.54 1.016 0))
      (text "-" (at 2.54 -0.762 0))
    )
    (symbol "CCVS_1_1"
      (pin passive line (at 2.54 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 2.54 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
    )
  )
  (symbol "CSW" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "W" (id 0) (at 0 5.08 0))
    (property "Value" "CSW" (id 1) (at 0 7.62 0))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 0))
    (property "Model" "<model name>" (id 4) (at 5.08 0 90))
    (property "Ctlvsrc" "<controlling vsrc>" (id 5) (at -5.08 -1.27 90))
    (property "ki_description" "Built-in current-controlled switch" (id 6) (at 0 0 0))
    (symbol "CSW_0_0")
    (symbol "CSW_0_1")
    (symbol "CSW_1_1"
      (pin passive line (at 2.54 3.81 270) (length 2.4384)
        (name "P")
        (number "1")
      )
      (pin passive line (at 2.54 -3.81 90) (length 2.4384)
        (name "N")
        (number "2")
      )
    )
  )
  (symbol "DIO" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (id 0) (at 0 2.54 0))
    (property "Value" "DIO" (id 1) (at 0 5.08 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Model" "<model name>" (id 4) (at 1.27 -2.54 0))
    (property "ki_description" "Built-in semiconductor diode" (id 5) (at 0 0 0))
    (symbol "DIO_0_1")
    (symbol "DIO_1_1"
      (pin passive line (at -3.81 0 0) (length 2.4384)
        (name "A")
        (number "1")
      )
      (pin passive line (at 3.81 0 180) (length 2.4384)
        (name "K")
        (number "2")
      )
    )
  )
  (symbol "INCLUDE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "INCLUDE" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Filename" "<file name>" (id 4) (at -10.16 -6.35 0))
    (property "Position" "top" (id 5) (at 10.16 1.27 0))
    (property "ki_description" "Include file" (id 6) (at 0 0 0))
    (symbol "INCLUDE_0_1")
  )
  (symbol "IND" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "L" (id 0) (at -1.27 0 90))
    (property "Value" "IND" (id 1) (at -3.81 0 90))
    (property "Footprint" "" (id 2) (at -3.81 -2.54 90))
    (property "Datasheet" "" (id 3) (at -1.27 0 90))
    (property "l" "<inductance>" (id 4) (at 2.54 0 90))
    (property "ki_description" "Built-in inductor" (id 5) (at 0 0 0))
    (symbol "IND_0_1")
    (symbol "IND_1_1"
      (pin passive line (at 0 3.81 270) (length 1.27)
        (name "1")
        (number "1")
      )
      (pin passive line (at 0 -3.81 90) (length 1.27)
        (name "2")
        (number "2")
      )
    )
  )
  (symbol "IND_COUPLING" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "K" (id 0) (at 0 6.35 0))
    (property "Value" "IND_COUPLING" (id 1) (at 0 8.89 0))
    (property "Footprint" "" (id 2) (at -2.54 0 0))
    (property "Datasheet" "" (id 3) (at 0 6.35 0))
    (property "Ind1" "<L1>" (id 4) (at -3.81 1.27 0))
    (property "Ind2" "<L2>" (id 5) (at 3.81 1.27 0))
    (property "k" "<factor>" (id 6) (at 0 3.81 0))
    (property "ki_description" "Built-in inductive coupling" (id 7) (at 0 0 0))
    (symbol "IND_COUPLING_0_1")
  )
  (symbol "ISRC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "I" (id 0) (at -3.81 0 90))
    (property "Value" "ISRC" (id 1) (at -6.35 0 90))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
    (property "Specification" "dc=0" (id 4) (at 3.81 0 90))
    (property "ki_description" "Built-in independent current source" (id 5) (at 0 0 0))
    (symbol "ISRC_0_0")
    (symbol "ISRC_1_1"
      (pin passive line (at 0 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 0 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
    )
  )
  (symbol "ISRC_NONLIN" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "B" (id 0) (at -3.81 0 90))
    (property "Value" "ISRC_NONLIN" (id 1) (at -6.35 0 90))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
    (property "i" "<expression>" (id 4) (at 3.81 0 90))
    (property "ki_description" "Built-in nonlinear controlled current source" (id 5) (at 0 0 0))
    (symbol "ISRC_NONLIN_0_0")
    (symbol "ISRC_NONLIN_1_1"
      (pin passive line (at 0 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 0 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
    )
  )
  (symbol "LIB" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "LIB" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Filename" "<file name>" (id 4) (at -10.16 -6.35 0))
    (property "Section" "<section>" (id 5) (at -10.16 -8.89 0))
    (property "Position" "top" (id 6) (at 10.16 1.27 0))
    (property "ki_description" "Include library section" (id 7) (at 0 0 0))
    (symbol "LIB_0_1")
  )
  (symbol "LOSSLESS_LINE" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "T" (id 0) (at 0 -2.54 0))
    (property "Value" "LOSSLESS_LINE" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at 0 -2.54 0))
    (property "Datasheet" "" (id 3) (at 0 -2.54 0))
    (property "td" "<delay>" (id 4) (at 0 -8.89 0))
    (property "z0" "<Z0>" (id 5) (at 0 -11.43 0))
    (property "ki_description" "Lossless transmission line" (id 6) (at 0 0 0))
    (symbol "LOSSLESS_LINE_0_0")
    (symbol "LOSSLESS_LINE_1_1"
      (pin input line (at -7.62 -5.08 0) (length 1.905)
        (name "I1")
        (number "1")
      )
      (pin input line (at -7.62 -7.62 0) (length 1.27)
        (name "I2")
        (number "2")
      )
      (pin input line (at 7.62 -5.08 180) (length 1.27)
        (name "O1")
        (number "3")
      )
      (pin input line (at 7.62 -7.62 180) (length 1.27)
        (name "O2")
        (number "4")
      )
    )
  )
  (symbol "LOSSY_LINE" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "O" (id 0) (at 0 -2.54 0))
    (property "Value" "LOSSY_LINE" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at 0 -2.54 0))
    (property "Datasheet" "" (id 3) (at 0 -2.54 0))
    (property "Model" "<model name>" (id 4) (at 0 -8.89 0))
    (property "ki_description" "Lossy transmission line" (id 5) (at 0 0 0))
    (symbol "LOSSY_LINE_0_0"
      (text "Lossy" (at 0 -5.08 0))
    )
    (symbol "LOSSY_LINE_1_1"
      (pin input line (at -7.62 -5.08 0) (length 1.905)
        (name "I1")
        (number "1")
      )
      (pin input line (at -7.62 -7.62 0) (length 1.27)
        (name "I2")
        (number "2")
      )
      (pin input line (at 7.62 -5.08 180) (length 1.27)
        (name "O1")
        (number "3")
      )
      (pin input line (at 7.62 -7.62 180) (length 1.27)
        (name "O2")
        (number "4")
      )
    )
  )
  (symbol "MODEL" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "MODEL" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Name" "<model name>" (id 4) (at -10.16 -6.35 0))
    (property "Type" "<device type>" (id 5) (at -10.16 -8.89 0))
    (property "Specification" "<model parameters>" (id 6) (at -10.16 -11.43 0))
    (property "ki_description" "Model definition" (id 7) (at 0 0 0))
    (symbol "MODEL_0_1")
  )
  (symbol "NJF" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 3.81 1.27 0))
    (property "Value" "NJF" (id 1) (at 5.08 3.81 0))
    (property "Footprint" "" (id 2) (at 5.08 3.81 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Model" "<model name>" (id 4) (at 3.81 -1.27 0))
    (property "ki_description" "Built-in NJFET transistor" (id 5) (at 0 0 0))
    (symbol "NJF_0_1")
    (symbol "NJF_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "D")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.334)
        (name "G")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "S")
        (number "3")
      )
    )
  )
  (symbol "NMF" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Z" (id 0) (at 3.81 1.27 0))
    (property "Value" "NMF" (id 1) (at 5.08 3.81 0))
    (property "Footprint" "" (id 2) (at 5.08 3.81 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Model" "<model name>" (id 4) (at 3.81 -1.27 0))
    (property "ki_description" "Built-in NMESFET transistor" (id 5) (at 0 0 0))
    (symbol "NMF_0_1")
    (symbol "NMF_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "D")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.334)
        (name "G")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "S")
        (number "3")
      )
    )
  )
  (symbol "NMOS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "M" (id 0) (at 5.08 5.08 0))
    (property "Value" "NMOS" (id 1) (at 5.08 7.62 0))
    (property "Footprint" "" (id 2) (at 5.08 7.62 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Model" "<model name>" (id 4) (at 5.08 2.54 0))
    (property "w" "<w>" (id 5) (at -1.27 5.08 0))
    (property "l" "<l>" (id 6) (at -1.27 2.54 0))
    (property "m" "<m>" (id 7) (at -1.27 -3.81 0))
    (property "ki_description" "Built-in NMOS transistor" (id 8) (at 0 0 0))
    (symbol "NMOS_0_1")
    (symbol "NMOS_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "D")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.334)
        (name "G")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "S")
        (number "3")
      )
      (pin input line (at 6.35 0 180) (length 5.08)
        (name "B")
        (number "4")
      )
    )
  )
  (symbol "NPN" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Q" (id 0) (at 3.81 1.27 0))
    (property "Value" "NPN" (id 1) (at 5.08 3.81 0))
    (property "Footprint" "" (id 2) (at 5.08 3.81 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Model" "<model name>" (id 4) (at 3.81 -1.27 0))
    (property "ki_description" "Built-in NPN transistor" (id 5) (at 0 0 0))
    (symbol "NPN_0_1")
    (symbol "NPN_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "C")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.715)
        (name "B")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "E")
        (number "3")
      )
    )
  )
  (symbol "OPAMP" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 0 5.08 0))
    (property "Value" "OPAMP" (id 1) (at 1.905 -5.08 0))
    (property "Footprint" "" (id 2) (at -2.54 -7.62 0))
    (property "Datasheet" "" (id 3) (at 0 5.08 0))
    (property "ki_keywords" "op amp amplifier operational" (id 4) (at 0 0 0))
    (property "ki_description" "Operational amplifier" (id 5) (at 0 0 0))
    (symbol "OPAMP_0_0"
      (text "+" (at -6.985 3.81 0))
      (text "-" (at -6.985 -3.81 0))
      (text "VDD" (at -3.81 3.81 900))
      (text "VSS" (at -3.81 -3.81 900))
    )
    (symbol "OPAMP_0_1")
    (symbol "OPAMP_1_1"
      (pin input line (at -10.16 3.81 0) (length 2.54)
        (name "+")
        (number "1")
      )
      (pin input line (at -10.16 -3.81 0) (length 2.54)
        (name "-")
        (number "2")
      )
      (pin output line (at 10.16 0 180) (length 2.54)
        (name "out")
        (number "3")
      )
      (pin input line (at -3.81 7.62 270) (length 2.921)
        (name "vdd")
        (number "4")
      )
      (pin input line (at -3.81 -7.62 90) (length 2.921)
        (name "vss")
        (number "5")
      )
    )
  )
  (symbol "OPAMP_DIFF" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at -1.905 5.715 0))
    (property "Value" "OPAMP_DIFF" (id 1) (at -1.905 -5.715 0))
    (property "Footprint" "" (id 2) (at -2.54 -7.62 0))
    (property "Datasheet" "" (id 3) (at 0 5.08 0))
    (property "ki_keywords" "op amp amplifier operational" (id 4) (at 0 0 0))
    (property "ki_description" "Operational amplifier (diff. output)" (id 5) (at 0 0 0))
    (symbol "OPAMP_DIFF_0_0"
      (text "+" (at -6.985 3.81 0))
      (text "+" (at 0.635 1.905 0))
      (text "-" (at -6.985 -3.81 0))
      (text "-" (at 0.635 -1.905 0))
      (text "VDD" (at -3.81 3.81 900))
      (text "VSS" (at -3.81 -3.81 900))
    )
    (symbol "OPAMP_DIFF_0_1")
    (symbol "OPAMP_DIFF_1_1"
      (pin input line (at -10.16 3.81 0) (length 2.54)
        (name "+")
        (number "1")
      )
      (pin input line (at -10.16 -3.81 0) (length 2.54)
        (name "-")
        (number "2")
      )
      (pin output line (at 10.16 2.54 180) (length 2.921)
        (name "out")
        (number "3")
      )
      (pin output line (at 10.16 -2.54 180) (length 2.921)
        (name "out")
        (number "4")
      )
      (pin input line (at -3.81 7.62 270) (length 2.921)
        (name "vdd")
        (number "4")
      )
      (pin input line (at -3.81 -7.62 90) (length 2.921)
        (name "vss")
        (number "5")
      )
    )
  )
  (symbol "OTA" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 2.54 6.35 0))
    (property "Value" "OTA" (id 1) (at 1.27 -6.35 0))
    (property "Footprint" "" (id 2) (at 1.27 -7.62 0))
    (property "Datasheet" "" (id 3) (at 3.81 5.08 0))
    (property "ki_keywords" "op amp amplifier transconductance operational" (id 4) (at 0 0 0))
    (property "ki_description" "Operational transconductance amplifier" (id 5) (at 0 0 0))
    (symbol "OTA_0_0"
      (text "+" (at -3.175 3.81 0))
      (text "-" (at -3.175 -3.81 0))
      (text "VDD" (at 0 4.445 900))
      (text "VSS" (at 0 -4.445 900))
    )
    (symbol "OTA_1_1"
      (pin input line (at -6.35 3.81 0) (length 2.54)
        (name "+")
        (number "1")
      )
      (pin input line (at -6.35 -3.81 0) (length 2.54)
        (name "-")
        (number "2")
      )
      (pin output line (at 6.35 0 180) (length 2.54)
        (name "out")
        (number "3")
      )
      (pin input line (at 0 7.62 270) (length 2.3876)
        (name "vdd")
        (number "4")
      )
      (pin input line (at 0 -7.62 90) (length 2.3876)
        (name "vss")
        (number "5")
      )
    )
  )
  (symbol "OTA_DIFF" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "X" (id 0) (at 2.54 6.35 0))
    (property "Value" "OTA_DIFF" (id 1) (at 1.27 -6.35 0))
    (property "Footprint" "" (id 2) (at 1.27 -7.62 0))
    (property "Datasheet" "" (id 3) (at 3.81 5.08 0))
    (property "ki_keywords" "op amp amplifier transconductance operational" (id 4) (at 0 0 0))
    (property "ki_description" "Operational transconductance amplifier (diff. output)" (id 5) (at 0 0 0))
    (symbol "OTA_DIFF_0_0"
      (text "+" (at -3.175 3.81 0))
      (text "+" (at 3.175 2.54 0))
      (text "-" (at -3.175 -3.81 0))
      (text "-" (at 3.175 -2.54 0))
      (text "VDD" (at 0 4.445 900))
      (text "VSS" (at 0 -4.445 900))
    )
    (symbol "OTA_DIFF_1_1"
      (pin input line (at -6.35 3.81 0) (length 2.54)
        (name "+")
        (number "1")
      )
      (pin input line (at -6.35 -3.81 0) (length 2.54)
        (name "-")
        (number "2")
      )
      (pin output line (at 6.35 2.54 180) (length 2.54)
        (name "o+")
        (number "3")
      )
      (pin output line (at 6.35 -2.54 180) (length 2.54)
        (name "o-")
        (number "4")
      )
      (pin input line (at 0 7.62 270) (length 2.3876)
        (name "vdd")
        (number "5")
      )
      (pin input line (at 0 -7.62 90) (length 2.3876)
        (name "vss")
        (number "6")
      )
    )
  )
  (symbol "OUTPUT_FILE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "OUTPUT_FILE" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Name" "<file name>" (id 4) (at -10.16 -6.35 0))
    (property "ki_description" "Define subcircuit" (id 5) (at 0 0 0))
    (symbol "OUTPUT_FILE_0_1")
  )
  (symbol "PARAM" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "PARAM" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Name" "<name>" (id 4) (at -10.16 -6.35 0))
    (property "Expression" "<expression>" (id 5) (at -10.16 -8.89 0))
    (property "ki_description" "Define new parameter" (id 6) (at 0 0 0))
    (symbol "PARAM_0_1")
  )
  (symbol "PJF" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at 3.81 1.27 0))
    (property "Value" "PJF" (id 1) (at 5.08 3.81 0))
    (property "Footprint" "" (id 2) (at 5.08 2.54 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Model" "<model name>" (id 4) (at 3.81 -1.27 0))
    (property "ki_description" "Built-in PJFET transistor" (id 5) (at 0 0 0))
    (symbol "PJF_0_1")
    (symbol "PJF_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "D")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.334)
        (name "G")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "S")
        (number "3")
      )
    )
  )
  (symbol "PMF" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Z" (id 0) (at 3.81 1.27 0))
    (property "Value" "PMF" (id 1) (at 5.08 3.81 0))
    (property "Footprint" "" (id 2) (at 5.08 2.54 0))
    (property "Datasheet" "" (id 3) (at 3.81 1.27 0))
    (property "Model" "<model name>" (id 4) (at 3.81 -1.27 0))
    (property "ki_description" "Built-in PMESFET transistor" (id 5) (at 0 0 0))
    (symbol "PMF_0_1")
    (symbol "PMF_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "D")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.334)
        (name "G")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "S")
        (number "3")
      )
    )
  )
  (symbol "PMOS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "M" (id 0) (at 5.08 5.08 0))
    (property "Value" "PMOS" (id 1) (at 5.08 7.62 0))
    (property "Footprint" "" (id 2) (at 5.08 6.35 0))
    (property "Datasheet" "" (id 3) (at 5.08 5.08 0))
    (property "Model" "<model name>" (id 4) (at 5.08 2.54 0))
    (property "w" "<w>" (id 5) (at -1.27 5.08 0))
    (property "l" "<l>" (id 6) (at -1.27 2.54 0))
    (property "m" "<m>" (id 7) (at -1.27 -3.81 0))
    (property "ki_description" "Built-in PMOS transistor" (id 8) (at 0 0 0))
    (symbol "PMOS_0_1")
    (symbol "PMOS_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "D")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.334)
        (name "G")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "S")
        (number "3")
      )
      (pin input line (at 6.35 0 180) (length 5.08)
        (name "B")
        (number "4")
      )
    )
  )
  (symbol "PNP" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "Q" (id 0) (at 3.81 1.27 0))
    (property "Value" "PNP" (id 1) (at 5.08 3.81 0))
    (property "Footprint" "" (id 2) (at 3.81 2.54 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Model" "<model name>" (id 4) (at 3.81 -1.27 0))
    (property "ki_description" "Built-in PNP transistor" (id 5) (at 0 0 0))
    (symbol "PNP_0_1")
    (symbol "PNP_1_1"
      (pin passive line (at 2.54 5.08 270) (length 2.54)
        (name "C")
        (number "1")
      )
      (pin input line (at -5.08 0 0) (length 5.715)
        (name "B")
        (number "2")
      )
      (pin passive line (at 2.54 -5.08 90) (length 2.54)
        (name "E")
        (number "3")
      )
    )
  )
  (symbol "RES" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (id 0) (at -2.54 0 90))
    (property "Value" "RES" (id 1) (at -5.08 0 90))
    (property "Footprint" "" (id 2) (at -1.778 0 90))
    (property "Datasheet" "" (id 3) (at 2.032 0 90))
    (property "r" "<resistance>" (id 4) (at 2.54 0 90))
    (property "ki_keywords" "r res resistor" (id 5) (at 0 0 0))
    (property "ki_description" "Built-in resistor" (id 6) (at 0 0 0))
    (symbol "RES_0_1")
    (symbol "RES_1_1"
      (pin passive line (at 0 3.81 270) (length 1.27)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -3.81 90) (length 1.27)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "RES_SEMI" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "R" (id 0) (at -5.08 0 90))
    (property "Value" "RES_SEMI" (id 1) (at -10.16 0 90))
    (property "Footprint" "" (id 2) (at -3.048 0 90))
    (property "Datasheet" "" (id 3) (at 3.302 0 90))
    (property "Model" "<model name>" (id 4) (at -2.54 0 90))
    (property "w" "<w>" (id 5) (at 2.54 0 90))
    (property "l" "<l>" (id 6) (at 5.08 0 90))
    (property "m" "<m>" (id 7) (at -7.62 0 90))
    (property "ki_keywords" "r res resistor" (id 8) (at 0 0 0))
    (property "ki_description" "Built-in semiconductor resistor" (id 9) (at 0 0 0))
    (symbol "RES_SEMI_0_1")
    (symbol "RES_SEMI_1_1"
      (pin passive line (at 0 3.81 270) (length 1.27)
        (name "~")
        (number "1")
      )
      (pin passive line (at 0 -3.81 90) (length 1.27)
        (name "~")
        (number "2")
      )
    )
  )
  (symbol "SUBCKT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "SUBCKT" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Name" "<name>" (id 4) (at -10.16 -6.35 0))
    (property "Pins" "<pin names>" (id 5) (at -10.16 -8.89 0))
    (property "ki_description" "Define subcircuit" (id 6) (at 0 0 0))
    (symbol "SUBCKT_0_1")
  )
  (symbol "SUBCKT_PARAM" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "SUBCKT_PARAM" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "Name" "<name>" (id 4) (at -10.16 -6.35 0))
    (property "Default" "<default value>" (id 5) (at -10.16 -8.89 0))
    (property "ki_description" "Define subcircuit parameter" (id 6) (at 0 0 0))
    (symbol "SUBCKT_PARAM_0_1")
  )
  (symbol "SUPPRESS_END" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "A" (id 0) (at -10.16 1.27 0))
    (property "Value" "SUPPRESS_END" (id 1) (at 0 -2.54 0))
    (property "Footprint" "" (id 2) (at 0 0 0))
    (property "Datasheet" "" (id 3) (at 0 0 0))
    (property "ki_description" "Suppress adding .end to netlist" (id 4) (at 0 0 0))
    (symbol "SUPPRESS_END_0_1")
  )
  (symbol "SW" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "S" (id 0) (at -3.81 0 90))
    (property "Value" "SW" (id 1) (at -6.35 0 90))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
    (property "Model" "<model name>" (id 4) (at 5.08 0 90))
    (property "ki_description" "Built-in voltage-controlled switch" (id 5) (at 0 0 0))
    (symbol "SW_0_0"
      (text "+" (at -1.27 1.27 0))
      (text "-" (at -1.27 -1.27 0))
    )
    (symbol "SW_0_1")
    (symbol "SW_1_1"
      (pin passive line (at 2.54 3.81 270) (length 2.4384)
        (name "P")
        (number "1")
      )
      (pin passive line (at 2.54 -3.81 90) (length 2.4384)
        (name "N")
        (number "2")
      )
      (pin input line (at -2.54 3.81 270) (length 2.4384)
        (name "CP")
        (number "3")
      )
      (pin input line (at -2.54 -3.81 90) (length 2.4384)
        (name "CN")
        (number "4")
      )
    )
  )
  (symbol "URC_LINE" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 -2.54 0))
    (property "Value" "URC_LINE" (id 1) (at 0 0 0))
    (property "Footprint" "" (id 2) (at 0 -2.54 0))
    (property "Datasheet" "" (id 3) (at 0 -2.54 0))
    (property "Model" "<model name>" (id 4) (at 1.27 -7.62 0))
    (property ";" "<length>" (id 5) (at 1.27 -10.16 0))
    (property "ki_description" "Uniform distributed RC line" (id 6) (at 0 0 0))
    (symbol "URC_LINE_0_0"
      (text "URC" (at 0 -5.08 0))
    )
    (symbol "URC_LINE_1_1"
      (pin input line (at -7.62 -5.08 0) (length 1.905)
        (name "I1")
        (number "1")
      )
      (pin input line (at 7.62 -5.08 180) (length 1.27)
        (name "I2")
        (number "2")
      )
      (pin input line (at 0 -8.89 90) (length 2.54)
        (name "GND")
        (number "3")
      )
    )
  )
  (symbol "VCCS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "G" (id 0) (at 0 5.08 0))
    (property "Value" "VCCS" (id 1) (at 0 7.62 0))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 0))
    (property "gain" "<gain>" (id 4) (at 6.35 0 90))
    (property "ki_description" "Built-in voltage-controlled current source" (id 5) (at 0 0 0))
    (symbol "VCCS_0_0"
      (text "+" (at -1.27 1.27 0))
      (text "-" (at -1.27 -1.27 0))
    )
    (symbol "VCCS_1_1"
      (pin passive line (at 2.54 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 2.54 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
      (pin input line (at -2.54 3.81 270) (length 1.905)
        (name "CP")
        (number "3")
      )
      (pin input line (at -2.54 -3.81 90) (length 1.905)
        (name "CN")
        (number "4")
      )
    )
  )
  (symbol "VCVS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "E" (id 0) (at 0 5.08 0))
    (property "Value" "VCVS" (id 1) (at 0 7.62 0))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 0))
    (property "gain" "<gain>" (id 4) (at 6.35 0 90))
    (property "ki_description" "Built-in voltage-controlled voltage source" (id 5) (at 0 0 0))
    (symbol "VCVS_0_0"
      (text "+" (at -1.27 1.27 0))
      (text "+" (at 2.54 1.016 0))
      (text "-" (at -1.27 -1.27 0))
      (text "-" (at 2.54 -0.762 0))
    )
    (symbol "VCVS_1_1"
      (pin passive line (at 2.54 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 2.54 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
      (pin input line (at -2.54 3.81 270) (length 1.905)
        (name "CP")
        (number "3")
      )
      (pin input line (at -2.54 -3.81 90) (length 1.905)
        (name "CN")
        (number "4")
      )
    )
  )
  (symbol "VSRC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "V" (id 0) (at -3.81 0 90))
    (property "Value" "VSRC" (id 1) (at -6.35 0 90))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
    (property "Specification" "dc=0" (id 4) (at 3.81 0 90))
    (property "ki_description" "Built-in independent voltage source" (id 5) (at 0 0 0))
    (symbol "VSRC_0_0"
      (text "+" (at 0 1.27 0))
      (text "-" (at 0 -1.27 0))
    )
    (symbol "VSRC_1_1"
      (pin passive line (at 0 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 0 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
    )
  )
  (symbol "VSRC_NONLIN" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
    (property "Reference" "B" (id 0) (at -3.81 0 90))
    (property "Value" "VSRC_NONLIN" (id 1) (at -6.35 0 90))
    (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
    (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
    (property "v" "<expression>" (id 4) (at 3.81 0 90))
    (property "ki_description" "Built-in nonlinear controlled voltage source" (id 5) (at 0 0 0))
    (symbol "VSRC_NONLIN_0_0"
      (text "+" (at 0 1.016 0))
      (text "-" (at 0 -0.762 0))
    )
    (symbol "VSRC_NONLIN_1_1"
      (pin passive line (at 0 3.81 270) (length 1.905)
        (name "P")
        (number "1")
      )
      (pin power_out line (at 0 -3.81 90) (length 1.905)
        (name "N")
        (number "2")
      )
    )
  )
)
