(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "pyopus:CAP" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at -3.81 0 90))
      (property "Value" "CAP" (id 1) (at -6.35 0 90))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 90))
      (property "Datasheet" "" (id 3) (at -3.81 0 90))
      (property "c" "<capacitance>" (id 4) (at 3.81 0 90))
      (property "ki_description" "Built-in capacitor" (id 5) (at 0 0 0))
      (symbol "CAP_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "CAP_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "pyopus:INCLUDE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 1.27 0))
      (property "Value" "INCLUDE" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Filename" "<file name>" (id 4) (at -10.16 -6.35 0))
      (property "Position" "top" (id 5) (at 10.16 1.27 0))
      (property "ki_description" "Include file" (id 6) (at 0 0 0))
      (symbol "INCLUDE_0_1"
        (rectangle (start -10.16 0) (end 10.16 -5.08)
          (fill (type none))
        )
      )
    )
    (symbol "pyopus:LIB" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 1.27 0))
      (property "Value" "LIB" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Filename" "<file name>" (id 4) (at -10.16 -6.35 0))
      (property "Section" "<section>" (id 5) (at -10.16 -8.89 0))
      (property "Position" "top" (id 6) (at 10.16 1.27 0))
      (property "ki_description" "Include library section" (id 7) (at 0 0 0))
      (symbol "LIB_0_1"
        (rectangle (start -10.16 0) (end 10.16 -5.08)
          (fill (type none))
        )
      )
    )
    (symbol "pyopus:OPAMP" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "X" (id 0) (at 0 5.08 0))
      (property "Value" "OPAMP" (id 1) (at 1.905 -5.08 0))
      (property "Footprint" "" (id 2) (at -2.54 -7.62 0))
      (property "Datasheet" "" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "op amp amplifier operational" (id 4) (at 0 0 0))
      (property "ki_description" "Operational amplifier" (id 5) (at 0 0 0))
      (symbol "OPAMP_0_0"
        (text "+" (at -6.985 3.81 0))
        (text "-" (at -6.985 -3.81 0))
        (text "VDD" (at -3.81 3.81 900))
        (text "VSS" (at -3.81 -3.81 900))
      )
      (symbol "OPAMP_0_1"
        (polyline
          (pts
            (xy -7.62 6.35)
            (xy -7.62 -6.35)
            (xy 7.62 0)
            (xy -7.62 6.35)
          )
          (fill (type none))
        )
      )
      (symbol "OPAMP_1_1"
        (pin input line (at -10.16 3.81 0) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin input line (at -10.16 -3.81 0) (length 2.54)
          (name "-")
          (number "2")
        )
        (pin output line (at 10.16 0 180) (length 2.54)
          (name "out")
          (number "3")
        )
        (pin input line (at -3.81 7.62 270) (length 2.921)
          (name "vdd")
          (number "4")
        )
        (pin input line (at -3.81 -7.62 90) (length 2.921)
          (name "vss")
          (number "5")
        )
      )
    )
    (symbol "pyopus:OUTPUT_FILE" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "A" (id 0) (at -10.16 1.27 0))
      (property "Value" "OUTPUT_FILE" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "Name" "<file name>" (id 4) (at -10.16 -6.35 0))
      (property "ki_description" "Define subcircuit" (id 5) (at 0 0 0))
      (symbol "OUTPUT_FILE_0_1"
        (rectangle (start -10.16 0) (end 10.16 -5.08)
          (fill (type none))
        )
      )
    )
    (symbol "pyopus:RES" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at -2.54 0 90))
      (property "Value" "RES" (id 1) (at -5.08 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "" (id 3) (at 2.032 0 90))
      (property "r" "<resistance>" (id 4) (at 2.54 0 90))
      (property "ki_keywords" "r res resistor" (id 5) (at 0 0 0))
      (property "ki_description" "Built-in resistor" (id 6) (at 0 0 0))
      (symbol "RES_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "RES_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "pyopus:VCVS" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "E" (id 0) (at 0 5.08 0))
      (property "Value" "VCVS" (id 1) (at 0 7.62 0))
      (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
      (property "Datasheet" "" (id 3) (at -5.08 -19.05 0))
      (property "gain" "<gain>" (id 4) (at 6.35 0 90))
      (property "ki_description" "Built-in voltage-controlled voltage source" (id 5) (at 0 0 0))
      (symbol "VCVS_0_0"
        (polyline
          (pts
            (xy 2.54 1.905)
            (xy 0.635 0)
            (xy 2.54 -1.905)
            (xy 4.445 0)
            (xy 2.54 1.905)
          )
          (fill (type none))
        )
        (text "+" (at -1.27 1.27 0))
        (text "+" (at 2.54 1.016 0))
        (text "-" (at -1.27 -1.27 0))
        (text "-" (at 2.54 -0.762 0))
      )
      (symbol "VCVS_1_1"
        (pin passive line (at 2.54 3.81 270) (length 1.905)
          (name "P")
          (number "1")
        )
        (pin power_out line (at 2.54 -3.81 90) (length 1.905)
          (name "N")
          (number "2")
        )
        (pin input line (at -2.54 3.81 270) (length 1.905)
          (name "CP")
          (number "3")
        )
        (pin input line (at -2.54 -3.81 90) (length 1.905)
          (name "CN")
          (number "4")
        )
      )
    )
    (symbol "pyopus:VSRC" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "V" (id 0) (at -3.81 0 90))
      (property "Value" "VSRC" (id 1) (at -6.35 0 90))
      (property "Footprint" "" (id 2) (at -6.858 -19.05 90))
      (property "Datasheet" "" (id 3) (at -5.08 -19.05 90))
      (property "Specification" "dc=0" (id 4) (at 3.81 0 90))
      (property "ki_description" "Built-in independent voltage source" (id 5) (at 0 0 0))
      (symbol "VSRC_0_0"
        (circle (center 0 0) (radius 1.905)
          (fill (type none))
        )
        (text "+" (at 0 1.27 0))
        (text "-" (at 0 -1.27 0))
      )
      (symbol "VSRC_1_1"
        (pin passive line (at 0 3.81 270) (length 1.905)
          (name "P")
          (number "1")
        )
        (pin power_out line (at 0 -3.81 90) (length 1.905)
          (name "N")
          (number "2")
        )
      )
    )
  )
  (junction (at 104.14 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 62.23) (diameter 0) (color 0 0 0 0))
  (junction (at 34.29 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 53.34 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 78.74 58.42) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 88.9 58.42) (xy 99.06 58.42)))
  (wire (pts (xy 76.2 58.42) (xy 78.74 58.42)))
  (wire (pts (xy 46.99 48.26) (xy 44.45 48.26)))
  (wire (pts (xy 104.14 58.42) (xy 110.49 58.42)))
  (wire (pts (xy 53.34 54.61) (xy 55.88 54.61)))
  (wire (pts (xy 50.8 54.61) (xy 53.34 54.61)))
  (wire (pts (xy 34.29 57.15) (xy 34.29 54.61)))
  (wire (pts (xy 88.9 68.58) (xy 88.9 71.12)))
  (wire (pts (xy 48.26 99.06) (xy 48.26 100.33)))
  (wire (pts (xy 104.14 58.42) (xy 104.14 60.96)))
  (wire (pts (xy 53.34 39.37) (xy 63.5 39.37)))
  (wire (pts (xy 62.23 66.04) (xy 62.23 68.58)))
  (wire (pts (xy 50.8 62.23) (xy 55.88 62.23)))
  (wire (pts (xy 34.29 99.06) (xy 34.29 100.33)))
  (wire (pts (xy 71.12 39.37) (xy 104.14 39.37)))
  (wire (pts (xy 53.34 54.61) (xy 46.99 48.26)))
  (wire (pts (xy 34.29 54.61) (xy 43.18 54.61)))
  (wire (pts (xy 78.74 58.42) (xy 88.9 58.42)))
  (wire (pts (xy 62.23 50.8) (xy 62.23 48.26)))
  (wire (pts (xy 30.48 54.61) (xy 34.29 54.61)))
  (wire (pts (xy 88.9 58.42) (xy 88.9 60.96)))
  (wire (pts (xy 104.14 39.37) (xy 104.14 58.42)))
  (wire (pts (xy 78.74 71.12) (xy 78.74 68.58)))
  (wire (pts (xy 99.06 58.42) (xy 99.06 60.96)))
  (wire (pts (xy 46.99 62.23) (xy 50.8 62.23)))
  (wire (pts (xy 50.8 62.23) (xy 50.8 64.77)))
  (wire (pts (xy 99.06 68.58) (xy 99.06 71.12)))
  (wire (pts (xy 53.34 39.37) (xy 53.34 54.61)))
  (wire (pts (xy 50.8 72.39) (xy 50.8 74.93)))
  (wire (pts (xy 78.74 60.96) (xy 78.74 58.42)))
  (wire (pts (xy 104.14 68.58) (xy 104.14 71.12)))
  (wire (pts (xy 34.29 64.77) (xy 34.29 67.31)))
  (wire (pts (xy 34.29 91.44) (xy 34.29 90.17)))
  (wire (pts (xy 48.26 91.44) (xy 48.26 90.17)))
  (text "Text1 position=top\n.param m1vt=0\n.param m1u0=0\n.param m2vt=0\n.param m2u0=0\n.param m3vt=0\n.param m3u0=0\n.param m4vt=0\n.param m4u0=0\n.param m5vt=0\n.param m5u0=0\n.param m6vt=0\n.param m6u0=0\n.param m7vt=0\n.param m7u0=0\n.param m8vt=0\n.param m8u0=0\n"
    (at 121.92 78.74 0)
  )
  (text "Text2 position=bottom\n.control\ndestroy all\ndelete all\n\ndc vin1 -0.9 0.9 lin 500\nplot v(out) vs v(inp,inn) xl -5m 2m\n\nset units=degrees\nac dec 100 1 1g\nplot db(v(out)/v(inp,inn)) unwrap(phase(v(out)/v(inp,inn)))\n.endc\n"
    (at 59.69 109.22 0)
  )
  (global_label "vdd" (shape input) (at 62.23 68.58 270) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "vss" (shape input) (at 62.23 48.26 90) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "in" (shape input) (at 30.48 54.61 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "inp" (shape input) (at 46.99 62.23 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "out" (shape input) (at 110.49 58.42 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "vdd" (shape input) (at 34.29 90.17 90) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "inn" (shape input) (at 44.45 48.26 180) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (global_label "vss" (shape input) (at 48.26 90.17 90) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 0 0 0))
  )
  (symbol (lib_id "pyopus:OPAMP") (at 66.04 58.42 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "X1" (id 0) (at 66.04 63.5 0))
    (property "Value" "" (id 1) (at 67.945 53.34 0))
    (property "Footprint" "" (id 2) (at 63.5 50.8 0))
    (property "Datasheet" "" (id 3) (at 66.04 63.5 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "pyopus:VSRC") (at 48.26 95.25 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Vss1" (id 0) (at 44.45 95.25 90))
    (property "Value" "" (id 1) (at 41.91 95.25 90))
    (property "Footprint" "" (id 2) (at 41.402 114.3 90))
    (property "Datasheet" "" (id 3) (at 43.18 114.3 90))
    (property "Specification" "dc=-0.9" (id 4) (at 52.07 95.25 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:VSRC") (at 34.29 95.25 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Vdd1" (id 0) (at 30.48 95.25 90))
    (property "Value" "" (id 1) (at 27.94 95.25 90))
    (property "Footprint" "" (id 2) (at 27.432 114.3 90))
    (property "Datasheet" "" (id 3) (at 29.21 114.3 90))
    (property "Specification" "dc=0.9" (id 4) (at 38.1 95.25 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:RES") (at 67.31 39.37 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 67.31 36.83 90))
    (property "Value" "" (id 1) (at 67.31 34.29 90))
    (property "Footprint" "" (id 2) (at 67.31 37.592 90))
    (property "Datasheet" "" (id 3) (at 67.31 41.402 90))
    (property "r" "1meg" (id 4) (at 67.31 41.91 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:RES") (at 46.99 54.61 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 46.99 52.07 90))
    (property "Value" "" (id 1) (at 46.99 49.53 90))
    (property "Footprint" "" (id 2) (at 46.99 52.832 90))
    (property "Datasheet" "" (id 3) (at 46.99 56.642 90))
    (property "r" "1meg" (id 4) (at 46.99 57.15 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "pyopus:VSRC") (at 50.8 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Vcom1" (id 0) (at 46.99 68.58 90))
    (property "Value" "" (id 1) (at 44.45 68.58 90))
    (property "Footprint" "" (id 2) (at 43.942 87.63 90))
    (property "Datasheet" "" (id 3) (at 45.72 87.63 90))
    (property "Specification" "dc=0" (id 4) (at 54.61 68.58 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 48.26 100.33 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR01" (id 0) (at 48.26 106.68 0))
    (property "Value" "" (id 1) (at 48.26 104.14 0))
    (property "Footprint" "" (id 2) (at 48.26 100.33 0))
    (property "Datasheet" "" (id 3) (at 48.26 100.33 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 34.29 100.33 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 34.29 106.68 0))
    (property "Value" "" (id 1) (at 34.29 104.14 0))
    (property "Footprint" "" (id 2) (at 34.29 100.33 0))
    (property "Datasheet" "" (id 3) (at 34.29 100.33 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 50.8 74.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR03" (id 0) (at 50.8 81.28 0))
    (property "Value" "" (id 1) (at 50.8 78.74 0))
    (property "Footprint" "" (id 2) (at 50.8 74.93 0))
    (property "Datasheet" "" (id 3) (at 50.8 74.93 0))
    (pin "1")
  )
  (symbol (lib_id "pyopus:VSRC") (at 34.29 60.96 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Vin1" (id 0) (at 30.48 60.96 90))
    (property "Value" "" (id 1) (at 27.94 60.96 90))
    (property "Footprint" "" (id 2) (at 27.432 80.01 90))
    (property "Datasheet" "" (id 3) (at 29.21 80.01 90))
    (property "Specification" "dc=0 ac=1" (id 4) (at 38.1 60.96 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 34.29 67.31 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 34.29 73.66 0))
    (property "Value" "" (id 1) (at 34.29 71.12 0))
    (property "Footprint" "" (id 2) (at 34.29 67.31 0))
    (property "Datasheet" "" (id 3) (at 34.29 67.31 0))
    (pin "1")
  )
  (symbol (lib_id "pyopus:OUTPUT_FILE") (at 38.1 26.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A1" (id 0) (at 27.94 25.4 0))
    (property "Value" "" (id 1) (at 38.1 29.21 0))
    (property "Footprint" "" (id 2) (at 38.1 26.67 0))
    (property "Datasheet" "" (id 3) (at 38.1 26.67 0))
    (property "Name" "topdc.cir" (id 4) (at 27.94 33.02 0))
  )
  (symbol (lib_id "pyopus:INCLUDE") (at 64.77 26.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A2" (id 0) (at 54.61 25.4 0))
    (property "Value" "" (id 1) (at 64.77 29.21 0))
    (property "Footprint" "" (id 2) (at 64.77 26.67 0))
    (property "Datasheet" "" (id 3) (at 64.77 26.67 0))
    (property "Filename" "miller.inc" (id 4) (at 54.61 33.02 0))
    (property "Position" "top" (id 5) (at 74.93 25.4 0))
  )
  (symbol (lib_id "pyopus:LIB") (at 91.44 26.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A3" (id 0) (at 81.28 25.4 0))
    (property "Value" "" (id 1) (at 91.44 29.21 0))
    (property "Footprint" "" (id 2) (at 91.44 26.67 0))
    (property "Datasheet" "" (id 3) (at 91.44 26.67 0))
    (property "Filename" "cmos180n.lib" (id 4) (at 81.28 33.02 0))
    (property "Section" "tm" (id 5) (at 81.28 35.56 0))
    (property "Position" "top" (id 6) (at 101.6 25.4 0))
  )
  (symbol (lib_id "pyopus:CAP") (at 78.74 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Cl1" (id 0) (at 74.93 64.77 90))
    (property "Value" "" (id 1) (at 72.39 64.77 90))
    (property "Footprint" "" (id 2) (at 79.7052 68.58 90))
    (property "Datasheet" "" (id 3) (at 74.93 64.77 90))
    (property "c" "1p" (id 4) (at 82.55 64.77 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 78.74 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR05" (id 0) (at 78.74 77.47 0))
    (property "Value" "" (id 1) (at 78.74 74.93 0))
    (property "Footprint" "" (id 2) (at 78.74 71.12 0))
    (property "Datasheet" "" (id 3) (at 78.74 71.12 0))
    (pin "1")
  )
  (symbol (lib_id "pyopus:INCLUDE") (at 118.11 26.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "A4" (id 0) (at 107.95 25.4 0))
    (property "Value" "" (id 1) (at 118.11 29.21 0))
    (property "Footprint" "" (id 2) (at 118.11 26.67 0))
    (property "Datasheet" "" (id 3) (at 118.11 26.67 0))
    (property "Filename" "mosmm.inc" (id 4) (at 107.95 33.02 0))
    (property "Position" "top" (id 5) (at 128.27 25.4 0))
  )
  (symbol (lib_id "pyopus:VCVS") (at 101.6 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "E1" (id 0) (at 101.6 59.69 0))
    (property "Value" "" (id 1) (at 101.6 57.15 0))
    (property "Footprint" "" (id 2) (at 94.742 83.82 90))
    (property "Datasheet" "" (id 3) (at 96.52 83.82 0))
    (property "gain" "1" (id 4) (at 107.95 64.77 90))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "power:GND") (at 104.14 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR06" (id 0) (at 104.14 77.47 0))
    (property "Value" "" (id 1) (at 104.14 74.93 0))
    (property "Footprint" "" (id 2) (at 104.14 71.12 0))
    (property "Datasheet" "" (id 3) (at 104.14 71.12 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 99.06 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR07" (id 0) (at 99.06 77.47 0))
    (property "Value" "" (id 1) (at 99.06 74.93 0))
    (property "Footprint" "" (id 2) (at 99.06 71.12 0))
    (property "Datasheet" "" (id 3) (at 99.06 71.12 0))
    (pin "1")
  )
  (symbol (lib_id "pyopus:RES") (at 88.9 64.77 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Rl1" (id 0) (at 86.36 64.77 90))
    (property "Value" "" (id 1) (at 83.82 64.77 90))
    (property "Footprint" "" (id 2) (at 87.122 64.77 90))
    (property "Datasheet" "" (id 3) (at 90.932 64.77 90))
    (property "r" "100meg" (id 4) (at 91.44 64.77 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 88.9 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR08" (id 0) (at 88.9 77.47 0))
    (property "Value" "" (id 1) (at 88.9 74.93 0))
    (property "Footprint" "" (id 2) (at 88.9 71.12 0))
    (property "Datasheet" "" (id 3) (at 88.9 71.12 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR08") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "A1") (unit 1) (value "OUTPUT_FILE") (footprint "")
    )
    (path
      (reference "A2") (unit 1) (value "INCLUDE") (footprint "")
    )
    (path
      (reference "A3") (unit 1) (value "LIB") (footprint "")
    )
    (path
      (reference "A4") (unit 1) (value "INCLUDE") (footprint "")
    )
    (path
      (reference "Cl1") (unit 1) (value "CAP") (footprint "")
    )
    (path
      (reference "E1") (unit 1) (value "VCVS") (footprint "")
    )
    (path
      (reference "R1") (unit 1) (value "RES") (footprint "")
    )
    (path
      (reference "R2") (unit 1) (value "RES") (footprint "")
    )
    (path
      (reference "Rl1") (unit 1) (value "RES") (footprint "")
    )
    (path
      (reference "Vcom1") (unit 1) (value "VSRC") (footprint "")
    )
    (path
      (reference "Vdd1") (unit 1) (value "VSRC") (footprint "")
    )
    (path
      (reference "Vin1") (unit 1) (value "VSRC") (footprint "")
    )
    (path
      (reference "Vss1") (unit 1) (value "VSRC") (footprint "")
    )
    (path
      (reference "X1") (unit 1) (value "miller") (footprint "")
    )
  )
)
