// Limiting of pn junction voltage (builtin pnjlim)

ground 0 

load "resistor.osdi"
load "simdiob.va"

model resistor resistor
model vsource vsource
model isource isource
model d simdio is=1e-12 n=1

v1 (1 0) vsource dc=1.0
d1 (1 0) d

control
  options op_debug=10 nr_debug=1
  options rawfile="binary" strictsave=1
  analysis op1 op 
endc

embed "simdiob.va" <<<FILE
`include "constants.vams"
`include "disciplines.vams"

module simdio(A,C);
    // Simplified SPICE diode, used for validation purposes
    
    // Terminals and internal nodes 
    inout A, C;
    electrical A,C;
    
    // Branches
    branch (A,C) br_a_c;
    
    // Model parameters
    (*desc = "Saturation current", units = "A"*) 
      parameter real Is = 1e-14 from [0:inf];
    (*desc = "Emission coefficient", units = ""*) 
      parameter real N = 1 from [0:inf];
    (*desc = "Flicker noise coefficient", units = ""*) 
      parameter real KF = 0 from [0:inf];
    (*desc = "Flicker noise exponent", units = ""*) 
      parameter real AF = 1 from [0:inf];
    (*desc = "Flicker noise frequency exponent", units = ""*) 
      parameter real EF = 1 from [0:inf];
    (*desc = "Debug messages", units = ""*) 
      parameter integer debug = 1 from [0:inf];

    // Output variables
    (*desc= "Diode ohmic current", units ="A" *) real Id;
    (*desc= "Differential conductance", units ="A/V" *) real gd;
    
    // Variables
    real Vfu, Vf, VT;
    real Tdev;
    
    analog begin
        // Device temperature and parameter measurement temperature (in K)
        Tdev = $temperature;
        
        // Thermal voltage
        VT = `P_K*Tdev/`P_Q;
        
        // Branch voltages
        Vfu = V(br_a_c);
        
        if (debug) begin 
            $debug("Tdev %.5e, VT %.12e, Vfu %.5e", Tdev, VT, Vfu);
            $debug("P_K %.12e, P_Q %.12e, Vfu %.5e", `P_K, `P_Q, Vfu);
        
            $display("Vf         %.5e", Vfu);
        end

        Vf = $limit(V(br_a_c), "pnjlim", $vt, 0.7);
        // Vf = Vfu;
        
        if (debug) begin
            $display("Vf limited %.5e", Vf);
        end
        
        // Ohmic current of diode branch
        Id = Is * (exp(Vf/(N*VT))-1);
        
        gd = ddx(Id, V(A));
        
        if (debug) begin
            $display("Id limited %.5e", Id);
            $display("gd limited %.5e", gd);
        end
        
        // Diode branch current
        I(br_a_c) <+ Id;

        // Shot noise
        I(br_a_c) <+ white_noise(2*`P_Q*abs(Id), "shot");

        // Flicker noise
        I(br_a_c) <+ flicker_noise(KF*pow(abs(Id), AF), EF, "flicker");

    end
endmodule

>>>FILE